# 3ae18c3b40a96211933a7326c352b7e

# HLM-8003EW Magnetic stirring high and low temperature thermostat

# 1、Application

HLM series magnetic stirring low-temperature reaction tank can be realized by low-temperature constant temperature or high-temperature constant temperature of the sample directly magnetic stirring, without the need for external installation of electric mixer for sample stirring, easy to use and safe. It is suitable for temperature control in chemical synthesis, testing of electronic components at different temperatures, and material testing.

 

**2、Features**

● Adopting two-stage compressor compound stack refrigeration technology, strong refrigeration, faster to reach the target temperature;

● Adopting PID temperature control with advanced proportional refrigeration control technology, which greatly improves the temperature stability;

● The magnetic stirrer inside the container is rotating, which can maintain the sample temperature uniformity and good precision for a long time;

● Adopting DC brushless motor with long life, trouble-free and infinitely adjustable speed;

● Alarm light and sound reminder at the same time, various alarm codes are displayed to determine the cause of the failure and repair methods;

● A variety of operating modes can be selected, accidental power failure can be automatically restored.

1. **Technical parameters**

|  |  |
| --- | --- |
| Product Model | HLM-8003EW |
| Product No. | 1032034001 |
| Tank volume (L) | 3 |
| Temperature range (℃) | -80~20 |
| Temperature stability (℃) | ±0.5 |
| Operating ambient temperature (℃) | 5~32 |
| Speed range (RPM) | 100~1200 |
| Speed regulation mode | Knob |
| Power supply voltage (V) | 200~230 |
| Display temperature mode | TFT |
| Setting mode | Touch Screen |
| Safety Protection | High Temperature Protection Over Temperature Protection |
| Heating power (W) | 750 |
| Cooling power(W) | 300 |
| Refrigeration capacity(W) | 400 |
| Refrigerant | R404A |
| Stirring sub size(MM) | φ8\*30 |
| Sink opening(MM) | Φ140 |
| Tank depth size(MM) | Φ165\*140 |
| Maximum capacity of reaction vessel | 500 |
| Maximum diameter of reaction vessel | ¢95 |
| Overall Dimension(MM)(W\*D\*H) | Φ106 |
| Packing size(MM)(W\*D\*H) | 500\*450\*370 |
| Net weight (kg) | 615\*565\*500 |
| Gross weight (kg) | 52 |

**4、Packing List**

|  |  |
| --- | --- |
| Name | Qty |
| Main unit | 1piece  |
| Retractable tank cover | 1piece  |
| Magnetic stirrer | 1piece |
| Vessel Clamp Column | 1 piece |
| Vessel clamp | 1 piece |
| Vessel Clamp Holder | 1 piece |
| Instruction manual | 1 piece  |